<config configVersion="1.1" device="PIC24FJ128GA010" coreVersion="4.65">
   <usedClasses class="java.util.HashMap">
      <entry>
         <string>System Module</string>
         <string>class com.microchip.mcc.mcu16.systemManager.DefaultSystemManagerMcu16</string>
      </entry>
      <entry>
         <string>Main Manager</string>
         <string>class com.microchip.mcc.mcu16.mainManager.MainManager</string>
      </entry>
      <entry>
         <string>JTAG</string>
         <string>class com.microchip.mcc.mcu16.systemManager.jtag.JTAG</string>
      </entry>
      <entry>
         <string>INTERNAL OSCILLATOR</string>
         <string>class com.microchip.mcc.mcu16.systemManager.clk.Clock</string>
      </entry>
      <entry>
         <string>IC1</string>
         <string>class com.microchip.mcc.mcu16.modules.ic.IC</string>
      </entry>
      <entry>
         <string>Pin Module</string>
         <string>class com.microchip.mcc.mcu16.pinManager.PinManager</string>
      </entry>
      <entry>
         <string>WATCHDOG</string>
         <string>class com.microchip.mcc.mcu16.systemManager.wdt.Wdt</string>
      </entry>
      <entry>
         <string>RESET</string>
         <string>class com.microchip.mcc.mcu16.systemManager.reset.RESET</string>
      </entry>
      <entry>
         <string>ICD</string>
         <string>class com.microchip.mcc.mcu16.systemManager.icd.Icd</string>
      </entry>
      <entry>
         <string>Interrupt Module</string>
         <string>class com.microchip.mcc.mcu16.interruptManager.InterruptManager</string>
      </entry>
      <entry>
         <string>com.microchip.mcc.mcu16.Mcu16PeripheralLibraryLibraryModule</string>
         <string>class com.microchip.mcc.protocolServices.base.modules.librarymodule.LibraryModule</string>
      </entry>
   </usedClasses>
   <usedLibraries class="java.util.ArrayList">
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.mcu16.Mcu16PeripheralLibrary" version="1.115"/>
   </usedLibraries>
   <tokenMap class="java.util.HashMap">
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllGraphicsSelect"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN2IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="FWPSA" alias="PR32"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RE2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="IESO"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN14IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name ENVREG"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN13IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM" alias="Simple Capture mode: Falling"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN9IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK"/>
         <value>out of lock</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+7.500%"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.875%"/>
         <value>51</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsOutput"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-6.000%"/>
         <value>48</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN6IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FCKSM" alias="CSDCMD"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefClkOutoutEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC"/>
         <value>FRCDIV</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_SOSC"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICI" alias="Every 2nd event"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="clock failure"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSwitching"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="FWPSA" alias="PR128"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscalerClock"/>
         <value>4000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-6.750%"/>
         <value>46</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICI" alias="Every 3rd event"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockTrim"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RE1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN0PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN11PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN6IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_USB"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Switch is Complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN18PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF"/>
         <value>no clock failure</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="ClockInput"/>
         <value>31000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="BKBUG" alias="OFF"/>
         <value>2048</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS512"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="IESO" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC" alias="LPRC"/>
         <value>1280</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscClock"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="PMPMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoOutputPinEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.125%"/>
         <value>53</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN21PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN16PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN19IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="RTCCMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM" alias="Simple Capture mode: Rising"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM" alias="Prescaler Capture mode: Every 16th rising"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="out of lock"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="I2C2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRIPLL"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="POSCMOD"/>
         <value>NONE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WINDIS"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG15" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="JTAGEN" alias="ON"/>
         <value>16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockSource"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+6.000%"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN19IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+5.625%"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN2IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN3IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.125%"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE"/>
         <value>1:8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN9PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefoClockDivSwitch"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RD14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RG14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="POSCMOD" alias="NONE"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG14" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-7.125%"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="POSCMOD" alias="HS"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="PMPMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSource"/>
         <value>FRC Oscillator</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN1PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN12PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN14IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="I2C2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler2"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="POSCMOD" alias="EC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK"/>
         <value>unlocked</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="locked"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T5MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FCKSM"/>
         <value>CSDCMD</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNIISRFunction"/>
         <value>ISR_Pin Module_CNI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+9.375%"/>
         <value>25</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC" alias="FRCDIV"/>
         <value>1792</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-8.625%"/>
         <value>41</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSource"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG13" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN15IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS16384"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN20PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN8IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+8.625%"/>
         <value>23</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="FWDTEN" alias="ON"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM" alias="Off"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SLEEP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T5MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_PRIMARY"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN2PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="GCP" alias="OFF"/>
         <value>8192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM"/>
         <value>Prescaler Capture mode: Every 4th rising</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC15"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="ICS"/>
         <value>PGx2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-5.250%"/>
         <value>50</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T5MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM" alias="Prescaler Capture mode: Every 4th rising"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.750%"/>
         <value>54</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC" alias="PRIPLL"/>
         <value>768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+8.250%"/>
         <value>22</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN14PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN3IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-7.500%"/>
         <value>44</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-9.000%"/>
         <value>40</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN1IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+6.750%"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC5MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+10.875%"/>
         <value>29</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WINDIS" alias="ON"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN0PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="JTAGEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN12IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN4PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN7IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="OSCIOFCN" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN6PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICBNE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="packageId"/>
         <value>TQFP100</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS4096"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN8PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC5MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICI_INT" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC" alias="FRCPLL"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.500%"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockChange"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICI" alias="Every 4th event"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF12" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN8PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.000%"/>
         <value>56</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICI"/>
         <value>Every</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN20PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN7IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfdivEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICI_INT" settingAlias="enable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN17PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureVcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPrescaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN7IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN16PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-9.750%"/>
         <value>38</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG10" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+10.125%"/>
         <value>27</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN18IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC5MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.000%"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.500%"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC" alias="PRI"/>
         <value>512</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN18IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG11" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN8PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN19PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="GWRP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG0"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN10PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockSource"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG12" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Request Switch"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRG15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN13PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG1"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.250%"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllTwoStagePostScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN14PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllEnable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN13IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="ICS" alias="PGx2"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="ICS" alias="PGx1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM" alias="Interrupt mode"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RG15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN18IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-10.500%"/>
         <value>36</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS1024"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN2IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN10PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG4"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG3"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN2PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center frequency"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.500%"/>
         <value>60</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN19IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC5MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.250%"/>
         <value>58</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="ROI" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG5"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN12PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.750%"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.750%"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG13" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD12" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRE3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="EXTR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllFeedbackDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CRCMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN6PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC15"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG6"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN7PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-11.25%"/>
         <value>34</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN14PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RG9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="no clock failure"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG15" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN13IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxPll"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN12PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG14" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG7"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN4PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN0IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="I2C2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN0PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RE9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UseSosc"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="IC1" registerAlias="ICCON1"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD12" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG11"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISC"/>
         <value>28702</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG8"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="TimerPeriod"/>
         <value>135.300s</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISB"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN15IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRIPLL"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG9"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="IESO" alias="ON"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG12"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISF"/>
         <value>12799</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN5PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Maximum frequency deviation"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="BKBUG"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet MCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISD"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN4IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISE"/>
         <value>1023</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="FWPSA"/>
         <value>PR128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="FWDTEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+7.875%"/>
         <value>21</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-4.500%"/>
         <value>52</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-6.375%"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="TRAPR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON"/>
         <value>1792</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.750%"/>
         <value>62</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN11IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="FWDTEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISA"/>
         <value>50943</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG10"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN16IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN8IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T2MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="GCP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN6IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV"/>
         <value>FRC/2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC2"/>
         <value>2000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN18PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG15"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICOV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN"/>
         <value>Switch is Complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllClock"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG9" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/256"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN21IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-8.250%"/>
         <value>42</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG8" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePoscErrataWorkaround"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+9.750%"/>
         <value>26</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc MCLR"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FRC"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC" alias="SOSC"/>
         <value>1024</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC"/>
         <value>FRCDIV</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG13"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICSIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+2.625%"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.125%"/>
         <value>61</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name MCLR"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISG"/>
         <value>62415</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+5.250%"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN19PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN8IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN20PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICOV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="clockSourceSelect"/>
         <value>CLOCK_LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG14"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN11IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC4MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="JTAGEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG6" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC5MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN15PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="IC1" name="IC1_ICI_INTISRFunction"/>
         <value>ISR_IC1_ICI_INT</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS"/>
         <value>PS32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC3MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="RESET" registerAlias="RCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="IC1" name="nonpps"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN5IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc ENVREG"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN17IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="BKBUG" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN6PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN17PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN17IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CRCMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet ENVREG"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RF12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T2MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICOV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+6.375%"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRF12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS8192"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockFBDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG7" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="SPI1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllPostScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN17IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN1IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN21IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="DOZE" alias="1:64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="CLKOStatusRestore"/>
         <value>RC15,input,ANSEL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="RTCCMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN12IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG3" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCF" settingAlias="ODF13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet ENVREG"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+9.000%"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN12IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockChange"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB12"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG5" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS2048"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IDLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="AD1PCFG"/>
         <value>192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG4" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN17PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCE" settingAlias="ODE2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV" settingAlias="RCDIV" alias="FRC/16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICI" alias="Every"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF12"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATD" settingAlias="LATD6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+7.125%"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATG" settingAlias="LATG6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKDIV"/>
         <value>12544</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCG" settingAlias="ODG12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="RTCCMD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CRCMD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN1IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN21IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPU2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN21PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG11" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="PMPMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS256"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICM" alias="Edge Detect Capture"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG1" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN10IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN1PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN3PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG0" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-7.875%"/>
         <value>43</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC5MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-9.375%"/>
         <value>39</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN3PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN14IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG7" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="OSCIOFCN" alias="OFF"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FNOSC" alias="FRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICBNE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPU1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG12" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATF" settingAlias="LATF12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+10.500%"/>
         <value>28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RG9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG2" alias="analog"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN5IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN5PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC"/>
         <value>FRCDIV</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICI_INT" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG5" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet MCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCDIV"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllCpuDivScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA15"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA14"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG10" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RF1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RE8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FCKSM" alias="CSECMD"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customViewerUpdate"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="FCKSM" alias="CSECME"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U1MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB8"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN10IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RD3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISG" settingAlias="TRISG1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WINDIS" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG6" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN9IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="POSCMOD" alias="XT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG9" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC3MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN7PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="IOPUWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAutoTune"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICBNE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN9PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+4.875%"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureUsb"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-3.375%"/>
         <value>55</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD3" settingAlias="CMPMD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN21PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN5IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-5.625%"/>
         <value>49</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="OC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICI_INT" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN2PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscaler"/>
         <value>1:2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN18PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="GCP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG8" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN4IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB12" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAvcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC3MD" alias="disabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN9IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.125%"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T4MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN16PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FailSafe"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSwitching"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_LPRC"/>
         <value>31000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+1.875%"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICTSEL"/>
         <value>TMR3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+3.375%"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="CONFIG2"/>
         <value>1955</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG1" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN11PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllDisplayScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-0.375%"/>
         <value>63</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN4PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="unlocked"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="LOCK" alias="in lock"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="CONFIG1"/>
         <value>14687</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="I2C1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD2" settingAlias="IC4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN20IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN7PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICSIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICSIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN16IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-2.625%"/>
         <value>57</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="ICD" name="customMasterSlaveViewerEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICTSEL" alias="TMR3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="IC1" registerAlias="ICCON1" settingAlias="ICTSEL" alias="TMR2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RE3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="SWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG2" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UI_OSCTUN_SETTING"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN13PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN10IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG0" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RF8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC12"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+0.375%"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN4IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISE" settingAlias="TRISE0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN9PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RF12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RG14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RF12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-10.875%"/>
         <value>35</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN15PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG2" settingAlias="OSCIOFCN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="WDTO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN3PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="ADC1MD"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN16IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD15"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG4" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS32768"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN3IE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN0IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN20IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN15PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN1PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-10.125%"/>
         <value>37</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN11PUE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-1.875%"/>
         <value>59</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN10PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency+11.250%"/>
         <value>30</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN15IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODC13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISF" settingAlias="TRISF1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="RESET" registerAlias="RCON" settingAlias="POR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center Frequency-11.625%"/>
         <value>33</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="U2MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODA15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN5PUE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Minimum frequency deviation"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="GWRP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPU2" settingAlias="CN19PUE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN11IE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="AD1PCFG" settingAlias="PCFG3" alias="digital"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PMD1" settingAlias="T4MD" alias="enabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FOSC"/>
         <value>4000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="GWRP" alias="OFF"/>
         <value>4096</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1" settingAlias="CN0IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATE" settingAlias="LATE3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN2" settingAlias="CN20IE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="CONFIG1" settingAlias="WDTPS" alias="PS1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISD" settingAlias="TRISD12"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="RESET" registerAlias="RCON" settingAlias="BOR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCD" settingAlias="ODD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPU1" settingAlias="CN13PUE" alias="disabled"/>
         <value>0</value>
      </entry>
   </tokenMap>
   <generatedFileHashHistoryMap class="java.util.HashMap">
      <entry>
         <file>mcc_generated_files\interrupt_manager.h</file>
         <hash>0cced0fc25f2e17bd326140542dd1b9d7094bfc1bb54ca5c7098acc178ed9174</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.h</file>
         <hash>61b59fd32de9659a5b4568ead8a187fa403b69305a803b0808bff8585f1b7854</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\ic1.c</file>
         <hash>e8c1f654f205bfffa76d73becf0ae01d44cf330564804219f548bdca2f62f8bc</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.c</file>
         <hash>4298cdcbdf3461dd22cfaa79ac7129dbb32c323c8216810cacc7f79b727d2163</hash>
      </entry>
      <entry>
         <file>main.c</file>
         <hash>f4e76f775cacf57e7438e94aab2389712c66077496d2b46f27baf3734c1cc7e1</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.h</file>
         <hash>9ca9665fc5749b8cde6fe361af2c4800c4f5ec8f8a99c6df23634af007c3df58</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\ic1.h</file>
         <hash>3e7925cef4a032bcc662aa84ae492976056feee57c6e489b78fd05f3430f9a8b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.h</file>
         <hash>5f0951170b8a9b433633c37a0487706f4e8e08b672249a6b62fe84bcde017e78</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.c</file>
         <hash>cbb4e4916880fea4a4eb0a4383031b53f98d9766f62e43f47f399257da81e8ce</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system.c</file>
         <hash>787dc4c7ad030532bd4ab09134bd871a16182128a7a4696aff03f83d0ada43da</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.c</file>
         <hash>e697b394a40352bf236d6d590a1c73fae95da984b6d1b4214524bc807ff75700</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\traps.h</file>
         <hash>8a9e44b548f93e6f5b5094271273b7bcbfe4811bf914a3306fee54f14bf3a7a8</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clock.h</file>
         <hash>f0da10f63a3d01d9474c7649da995839b64d087f33467bd35f793ed958bd72bc</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\interrupt_manager.c</file>
         <hash>80071d9b92d2742dd0cfdbe770128d5ea73ba550c89ee9b6de06851a347f5e4d</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.c</file>
         <hash>01f0fc2e44e3e65227d25e0e2c3c25702bc34bd45218804118fa13086f4d0687</hash>
      </entry>
   </generatedFileHashHistoryMap>
</config>